energy/TeV -1 10 1 10^210^310^410

-1 s^{-2} integral flux sensitivity / erg cm

-14 10

-13 10

-12 10

-11 10

-10 10

-9 10 KASCADE U.L. H.E.S.S. survey, hard sources MGRO J1908+06 HESS J1908+06

HiSCORE

2 10 km

2 100 km

CTA point-source, 50 hours HAWC point-source, 5 years LHAASO point-source, 1 year )ν IceCube Milagro sources, 5 years (